|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 50. Remarks: Zu\* 11: 883  -  -  -  -  Alternative Types: 205/50 R17 89V  225/45 R17 91W  225/40 R18 92V M+S A: 225/35 R19 88Y  A: 225/40 R18 88Y A: 225/35 R19 88Y  -  -  51. Esemptions: | P: 245/30 R19 89Y  P: 245/35 R18 88Y  P: 245/30 R19 89Y | **CdS – DATA SHEET**  **for complete vehicles.**  0.1. Make: 0.2. Type:  Variant: Version:  0.2.1. Commercial name (s): 0.4. Category:  0.5. Name and address of manufacturer  of the base vehicle: 0.6. Manufacturer address: | |  |  |  | | --- | --- | --- | | **{{A1}}**  **{{A2}}**  **{{A3}}**  **{{A4}}**  **{{A5}} {{A6}}** | **(D.1) (D.2) (D.2) (D.2)**  **(D.3) (J)** |  |   **{{A7}}** | |
| **Muenchen 13 Germany**  Vehicle identification number: **WBA1C7104FJ953345 (E)**  Location of the Vehicle Identification Number: **under the right front seat, A-, B-pillar, in the engine compartment (12)**  with the implication **e1\*2007/46\*0283\*12 (K)** given on **11-06-2014 (3-4 meses antes** type described in all respects. **letra B del doc)** | | | | |
| **CdS-\*\*\*\*/0\*** | |  | | Date: 29/06/2022 |

**The data on this document is obtained from a database search. The information may differ from the state of vehicle. No physical inspection of the vehicle was performed.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1. Number of axles / wheels:  2. Powered axles:  3. Wheelbase :(mm)  5. Axle(s) track – 1/ 2: (mm)  6.1. Length:(mm) 7.1. Width:(mm)  8. Height:(mm)  11. Rear overhang:(mm)  12.1. Mass of the vehicle with bodywork in running order:(kg) 14.1. Technically permissable maximum laden mass:(kg)  14.2. Distribution of this mass among the axles – 1 / 2:(kg) 14.3. Technically perm. max mass on each axle – 1 / 2:(kg)  16. Maximum permissible roof load:(kg)  17. Maximum mass of trailer – braked / unbraked:(kg)  18. Maximum mass of combination:(kg)  19.1. Maximum vertical load at the coupling point for a trailer:(kg)  20. Engine manufacturer:  21. Engine code as marked on the engine:  22. Working principle: 22.1. Direct injection:  23. Pure electric:  23.1 Hybrid [electric] vehicle:  24. Number and arrangement of cylinders:  25. Capacity:( cm3)  26. Fuel:  27. Maximum net power:( kW/min -1)  28. Clutch (type):  29. Gearbox (type):  29.1. Gear: | {{B1}}/{{B2}}  {{B3}}  {{B4}}  {{B5}}  {{B6}}  1765 (41)  1421 (42)  869 (43)  1320 (G)  1885 (F.1-F.2) (53)  880/1090 (N.1/N.2) (54 V/B)  880/1090 (N.1/N.2) (54)  75 (55)  1200/690 (O.1/O.2) (57/58)  3160 (F.3) (66)  75 (Z) (67)  BMW (25)  N47D20C (P.5) (25) Common rail   |  |  | | --- | --- | | No  No  No  4, In line 1995  Diesel  85/4000 | (26)  (P.1) (27) (P.3)  (P.2/P.4) (28) |   Single plate dry Manual (18) 6 (18) | 30. Final drive ratio: 3.08 (18)  32. Tyres and wheels:  Tyres on wheels 1: 195/55 R16 87H (68/69/70)  Tyres on wheels 2: 195/55 R16 87H (68/69/70)  34. Steering, method of assistance: Electric Steering  35. Brief description of the braking system: Double wishbone/Multi-link independent Ventilated discs /Disc  ABS  37. Type of body: Hatchback  38. Colour of vehicle: White (R)  [41. Number and configuration of doors: 5 (38)](#bookmark1)  [42.1. Number and position of seats: 5 (S.1) (37)](#bookmark2)  [43.1. EC type approval mark of couplind device E13 00-3368 (56)](#bookmark3)  if fitted:  44. Maximum speed:(km/h) 200 (T) (19)  45. Sound level:  Stationary (dB(A)) at engine speed (min-1) 76 at 3000 (U.1/U.2)  Drive-by (dB(A)): 73 (U.3)  46. Emissions standard: EURO 5 (V9)  46.1. Exhaust emission: 715/2007\*195/2013J (V9)  CO (g/km): 0.2393 - - - -  HC (g/km): - - - - - - - -  NOX (g/km): **toda la tabla esta en el 72** 0.1246 - - - -  HC+NOX (g/km): 0.1546 - - - -  k – value (g/km): - - - - - - - -  Particulates (g/km): 0.00032 - - - -  46.2 Smoke (corrected value of the absorption coefficient)  47. CO2 emissions/fuel consumption NEDC values: | | | - - - -  - - - -  - - - -  - - - -  - - - -  - - - -  0.51 m-1 |
| |  |  |  | | --- | --- | --- | | urban conditions:  extra-urban conditions: combined: | CO2(g/km) 129  100  114 (V.7) | Fuel consumption (l/100km)  5.3  3.8  4.3 |   47.1. CO2 emissions/fuel consumption WLTP values:  CO2(g/km) Fuel consumption (l/100km) | | | |
| Low:  Medium High:  Maximum value Combined  Weighted combined | -  -  -  -  -  - | -  -  -  -  -  - | |
| 47.2. Pure electric vehicles and externally rechargeable Hybrid electric vehicles: Power consumption weighted/combined  **-** Wh/km  Electrical range **-** km | | | |